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A Nothing found, sorry!

No ‘RFspace CloudIQ, CloudSDR, NetSDR, SDR-IP* radios were found.

—> Help
Display the online radio support pages

—> Firewall

Show the Windows firewall (opens a new window)

- Logfile

Show program logfile (opens a new window)

() Show the checKlist. oK
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Show these options
[] converter selection

[invert spectrum

Address Option | DIl
192.168.4.31::50000 RFspace001
SDR-IQ #HV001078 RFspace002
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Default

SDR Console v3.2
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Al Local & Server

Name Model | Frequency | Serial Address
Cloud SOR  SDRP 0-50MHz ~ CS000131  192.168.4.31::50000
SDRIQ  SDRIQ 0-30MHz HVO01078  SDR-IQ #HV001078

Bandwidth: |190 kHz

Freq: 7.039.3 MHz
Span: +2.325 kHz
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